LAB 3

|  |  |
| --- | --- |
|  | |
| Instructions |  |
| 1.0 Install a DHCP Server by Powershell  2.0 Create a new Scope called VLAN1 192.168.1.0  3.0 Create a new range of 192.168.1.1-192.168.1.254  4.0 Exclude the first 15 IP addresses 192.168.1.1-192.168.1.15  5.0 Authorize the server to run in an ADDS  6.0 Ensure the DHCP Server lease IP address.  **NOTE:** Everything must be done by **PowerShell**   1. Print screen of DHCP Server is installed     2.0 Print Screen of Scope is called VLAN10      3.0 Print Screen of a new Range 192.168.1.1-192.168.1.254      4.0 Print Screen of DHCP server is authorized in ADDS    5.0 Print Screen of Users leasing | |